TECHNICAL SPECIFICATION
CCTV AND ALARM EQUIPMENT
	Buyer / organisation
	…

	Subject
	Purchase of CCTV and Alarm Equipment

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the cctv and alarm equipment listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 30 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	IP dome camera
	Resolution, lens focal length, IR range and IP/IK rating stated, ONVIF Profile T conformant
	Each
	

	2
	IP bullet camera
	Resolution, lens focal length, IR range and IP rating stated, ONVIF Profile T conformant
	Each
	

	3
	PTZ camera
	Optical zoom, pan and tilt range, preset count stated, ONVIF Profile T conformant
	Each
	

	4
	Fisheye camera
	Resolution, field of view and dewarping support stated, ONVIF Profile T conformant
	Each
	

	5
	Thermal camera
	Sensor resolution, lens and detection range stated, ONVIF Profile T conformant
	Each
	

	6
	Low light camera
	Minimum illumination in lux and colour retention stated, ONVIF Profile T conformant
	Each
	

	7
	Network video recorder
	Channel count, throughput, disk bays and PoE ports stated, ONVIF Profile T client conformance
	Each
	

	8
	Surveillance grade hard disk
	Capacity, workload rating and continuous duty stated
	Each
	

	9
	PoE switch
	Port count, PoE standard (802.3af/at/bt) and total power budget
	Each
	

	10
	PoE injector
	PoE standard and output power stated
	Each
	

	11
	Uninterruptible power supply
	VA and W rating, topology and runtime stated
	Each
	

	12
	CAT6 cable
	Solid or stranded, shielding, sheath rating and drum length
	Box
	

	13
	RJ45 connector and keystone jack
	Category, shielding and termination method stated
	Each
	

	14
	Camera bracket and housing
	Load capacity, IP rating and cable management stated
	Each
	

	15
	Camera pole
	Height, wall thickness, base plate and coating stated
	Each
	

	16
	Junction box and trunking
	IP rating, dimensions and material stated
	Each
	

	17
	Alarm control panel
	Zone count, expansion capability and grade stated
	Each
	

	18
	Alarm keypad
	Display type, wired or wireless and user code capacity
	Each
	

	19
	Communication module, GSM or IP
	Transmission path, dual path option and reporting protocol
	Each
	

	20
	PIR motion detector
	Coverage in m, pet immunity and mounting height stated
	Each
	

	21
	Curtain and outdoor detector
	Coverage pattern, IP rating and anti-masking stated
	Each
	

	22
	Magnetic door or window contact
	Gap distance, surface or flush mount stated
	Each
	

	23
	Glass break and shock detector
	Coverage radius and sensitivity adjustment stated
	Each
	

	24
	Smoke and gas detector, alarm connected
	Detection principle and interconnection method stated
	Each
	

	25
	Indoor and outdoor sounder
	Sound level in dB, strobe option and tamper protection
	Each
	

	26
	Access control card reader
	Credential technology, read range and IP rating stated
	Each
	

	27
	Electric lock, magnet or strike
	Holding force, fail-safe or fail-secure and voltage stated
	Each
	

	28
	Access control panel and credentials
	Door count, user capacity and credential type stated
	Each
	

	29
	Turnstile and barrier
	Passage width, throughput and fail-safe operation stated
	Each
	

	30
	CCTV and alarm maintenance kit
	Lens cleaning, connectors, spare fixings; contents listed
	Set
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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